



**A Series HD Wi-Fi Network Camera Quick Start Guide**

**V 1.0.1**



# Packing List

** **


Device × 1 QSG ×1

** **

Power Adapter ×1 Screw Package ×1

Quick Installation Board ×1 Installation Position Map×1

****

USB ×1

# Product Appearance



** **

Figure 2-1 Figure 2-2


****

Figure 2-3

Please refer to the following sheet for more details about each port.

| **SN** | **Name** |
| --- | --- |
| 1 | Lens |
| 2 | MIC |
| 3 | Reset/WPS (Wi-Fi Protected Setup) button |
| 4 | Micro SD card slot |
| 5 | Network port |
| 6 | Power port |
| 7 | Indicator light |
| 8 | Loudspeaker |

Sheet 2-1

**Note:**

For reset, long press for 8 seconds and then the light off; For WPS (Wi-Fi Protected Setup) one quick press.

Please refer to the following sheet for more details about status of indicator light.

|  |  |
| --- | --- |
| **Device status** | **Indicate light status** |
| Red light spinning | Booting, device malfunction, fail to boot up |
| Green light spinning | Booting completed, await wifi config, enter smart config status; |
| Green light breathing | Wifi smart config in progress, including WPS (Wi-Fi Protected Setup),  management frame and etc. |
| Blue light normally on | Wifi connection succeeded, operate normally. |
| Blue light flashing | Device upgrade |
| Yellow light breathing | Network connection failure or disconnection after network connection success. |
| Red light breathing | Alarm or SD card malfunction |

Sheet 2-2

# Operate by EasyViewer

**Step 1**

Power on the camera.

**Step 2**

Connect iphone to a WiFi signal.

**Step 3**

Open EasyViewer (downloaded from APP Store), choose Device Manager.


****

Figure 3-1

**Step 4**

Please select “P2P” when the network cable is connected, select “WiFi configuration” for wireless connection. Here is an example of wireless connection.


****

Figure 3-2

**Step 5**

Input a device name and scan the QR code (on the bottom of the device chassis) on camera, then “next”.


****

Figure 3-3

**Step 6**

Input the WiFi password, then “next”.


****

Figure 3-4

Step 7

Connection succeeds.




**  **

Figure 3-5 Figure 3-6 Figure 3-7

**Note:**

Please try again or check the WiFi password if it failed.

The WiFi configuration will be closed if activating WPS (WI-FI Protected Setup) function; Please reset the device if you still need to configure WiFi via EasyViewer.

# Device Installation

**Important**

Before the installation, please make sure the installation environments can at least support 3x weight of the camera.


****

Figure 4-1

**Note:**

* **This quick start guide is for reference only. Slight difference may be found in user interface.**
* **All the designs and software here are subject to change without prior written notice.**
* **All trademarks and registered trademarks mentioned are the properties of their respective   
  owners.**
* **If there is any uncertainty or controversy, please refer to the final explanation of us.**
* **Please visit our website or contact your local service engineer for more information.**